From Christian Kirsch : christian.ck.kirsch@fau.de
Note that these files require the newest SIMPUT (2.5.0) and SIXTE (2.7.0) versions to run.
   To use the files, simply unpack it like the X-IFU instrument files on the web (instructions at https://www.sternwarte.uni-erlangen.de/research/sixte/simulation.php).
To run simulations in xifupipeline, users will have to specify two XML files via the parameters XMLFile and AdvXml. The available files are:
XMLFile:  - xifu_baseline.xml (In-focus file with 5” PSF, newest (v3.1) PSF and vignetting)   xifu_baseline_filter.xml (Same as above, with 100um Be Filter ARF)   xifu_baseline_degr10.xml (In-focus file with degraded, 10” PSF, newest (v3.1) PSF and vignetting)   xifu_baseline_filter_degr10.xml (Same as above, with 100um Be Filter ARF)   xifu_baseline_35mm.xml (35mm defocusing, with newest (v3.1) PSF)  - xifu_baseline_filter_35mm.xml (Same as a bove, with 100um Be Filter ARF)
AdvXml:  - xifu_detector_lpa25_tdm_33_317um_20211029.xml (Newest pitch and crosstalk matrices)  - xifu_detector_lpa25_tdm_33_275um_20211103.xml (Old pitch, new crosstalk matrices)
 If there’s any questions, don’t hesitate to ask.
Best, hristian